commit f90124c73edd050b24961197a4abcf17e53b41a8
Author: Jaroslav Kysela <perex@perex.cz>
Date:   Thu Nov 14 09:38:49 2024 +0100

    alsactl: 90-alsa-restore.rules - fix alsa_restore_go/std
    
    Fix the label mismatch which was introduced in the transition from the
    temporary test rules.
    
    Closes: https://github.com/alsa-project/alsa-utils/issues/280
    Fixes: 8116639 ("alsactl: 90-alsa-restore.rules - add support for AMD ACP digital microphone")
    Signed-off-by: Jaroslav Kysela <perex@perex.cz>

diff --git a/alsactl/90-alsa-restore.rules.in b/alsactl/90-alsa-restore.rules.in
index 85f0b15..dae2ed8 100644
--- a/alsactl/90-alsa-restore.rules.in
+++ b/alsactl/90-alsa-restore.rules.in
@@ -3,6 +3,8 @@
 ACTION=="add", SUBSYSTEM=="sound", KERNEL=="controlC*", KERNELS!="card*",@extratest@ GOTO="alsa_restore_go"
 GOTO="alsa_restore_end"
 
+LABEL="alsa_restore_go"
+
 ENV{ALSA_CARD_NUMBER}="$attr{device/number}"
 
 # mark HDA analog card; HDMI/DP card does not have capture devices
@@ -21,7 +23,7 @@ TEST!="/run/udev/alsa-hda-analog-card", GOTO="alsa_restore_std"
 IMPORT{program}="/usr/bin/cat /run/udev/alsa-hda-analog-card"
 ENV{ALSA_CARD_HDA_ANALOG}!="", ENV{ALSA_CARD_NUMBER}="$env{ALSA_CARD_HDA_ANALOG}"
 
-LABEL="alsa_restore_go"
+LABEL="alsa_restore_std"
 TEST!="@daemonswitch@", RUN+="@sbindir@/alsactl@args@ restore $env{ALSA_CARD_NUMBER}"
 TEST=="@daemonswitch@", RUN+="@sbindir@/alsactl@args@ nrestore $env{ALSA_CARD_NUMBER}"
 
